diff --git a/drivers/tty/vt/vt.c b/drivers/tty/vt/vt.c
index 693091ab7..ada523ccf 100644
--- a/drivers/tty/vt/vt.c
+++ b/drivers/tty/vt/vt.c
@@ -159,7 +159,7 @@ static void set_palette(struct vc_data *vc);
 static int printable;		/* Is console ready for printing? */
 int default_utf8 = true;
 module_param(default_utf8, int, S_IRUGO | S_IWUSR);
-int global_cursor_default = -1;
+int global_cursor_default = 0;
 module_param(global_cursor_default, int, S_IRUGO | S_IWUSR);
 
 static int cur_default = CUR_DEFAULT;
@@ -176,7 +176,7 @@ int console_blanked;
 
 static int vesa_blank_mode; /* 0:none 1:suspendV 2:suspendH 3:powerdown */
 static int vesa_off_interval;
-static int blankinterval = 10*60;
+static int blankinterval = 0;
 core_param(consoleblank, blankinterval, int, 0444);
 
 static DECLARE_WORK(console_work, console_callback);
diff --git a/kernel/sched/core.c b/kernel/sched/core.c
index 5e973efc0..2e3334726 100644
--- a/kernel/sched/core.c
+++ b/kernel/sched/core.c
@@ -286,7 +286,7 @@ const_debug unsigned int sysctl_sched_time_avg = MSEC_PER_SEC;
  * period over which we measure -rt task cpu usage in us.
  * default: 1s
  */
-unsigned int sysctl_sched_rt_period = 1000000;
+unsigned int sysctl_sched_rt_period = 100000;
 
 __read_mostly int scheduler_running;
 
@@ -294,7 +294,7 @@ __read_mostly int scheduler_running;
  * part of the period that we allow rt tasks to run in us.
  * default: 0.95s
  */
-int sysctl_sched_rt_runtime = 950000;
+int sysctl_sched_rt_runtime = 95000;
 
 /*
  * __task_rq_lock - lock the rq @p resides on.
